# danWand

# Quick Setup Guide

1. Connect the device to power with a standard USB cable
   1. The device will startup and blink red (one day in the future) when ready to connect to
   2. The device will create an Access Point with SSID danWand and passphrase danwandpassword
2. Connect a device (mobile phone, tablet, PC) to the access point
3. Connect a browser to the device
   1. Website: <http://192.168.11.1> (danwandconfig.local)
4. Login to the device
   1. Userid: admin
   2. Password: password
5. Select the Wi-Fi Administrations Menu
   1. Under “Connect new WIFI”
   2. Enter SSID and passphrase for your Wi-Fi Network
   3. Save information
   4. Reboot Device